Offline
I2C Target
Connect to a conucon input module to route GCode.
Unknown
X: 0.000
|
Y: 0.000
|
Z: 0.000
F mm/m
1

### Controller Settings

FW: --
GUI: v1.0.0
Machine
Auto-save on Enter or focus loss
Loading settings...
No I2C scan data yet.
Settings count: 0 I2C count: 0
> conucon engineering v1.0.0: System initialized. Ready to connect...

### Select Microcontroller

Choose target hardware for firmware flashing.

### Connect

Connect via USB serial or enter the controller's IP address.

### Mask Editor

Choose axes to include in this mask.

Value: 0 Binary: 0b0000